Variable CSPMail::Port Description: The TCP/IP port of the SMTP server.
| Prototype unsigned short Port; Remarks: The default value is "25". In order to send the mail you must call the member function Send(). See also: member function Send() member variables MailServer, To, SenderAddr, MailServer
CSPMail | Other support classes | Class Categories | Online help home | Back
www.micronovae.com Copyright © 2002 - 2004 Micronovae Ltd